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In the schematic above you can see Santiago’s hand written component values for the parts that Frank Levi added to Slash’s JCM 800 to create the #34 mod.

[image: image2.png]PCBs JHBO

Vi.21 ECCH3, f)loment
supaly shoun an powsy

stoge dlagrom.

X
aQ
a
=
o~
Pl
o

Trebla
Unpk ‘Rl

RS W70k

VRL 1M leog

Preawp Yol

Flie:1 2203PRE .0GM





JCM 800 2203/2204 preamp section diagram 
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JCM 800 2203/2204 power amp section diagram
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